"Symbol";"Value";"Unit";
"Clamping_range_4_amount";"2";"";
"Surface_roughness_ISO_4287";"Ra = 0,421 μm";"";
"Clamping_range_4_max";"12.5 mm";"";
"IP_protection_class";"IP54, IP55, IP64, IP65, IP66, IP67, IP68";"";
"Clamping_range_4_min";"8 mm";"";
"For_max_number_of_cables";"21";"";
"Max_cable_d";"12.5 mm";"";
"Length";"147 mm";"";
"Mounting_height";"14 mm";"";
"Clamping_range_2_max";"7.5 mm";"";
"Clamping_range_2_min";"4 mm";"";
"Clamping_range_3_amount";"4";"";
"Clamping_range_2_amount";"14";"";
"Clamping_range_3_min";"5.5 mm";"";
"SUPPLIER";"icotek GmbH & Co. KG";"";
"Clamping_range_1_amount";"1";"";
"REFERENCE";"73930";"";
"TraceParts.PartTitle";"KEL-DPU-HD 24";"";
"TraceParts.InstanceId";"90-23052025-045160CERYB9ALZKSL9T6XGMT5XJAKT";"";
"Height";"14 mm";"";
"Clamping_range_1_max";"6.3 mm";"";
"Part_Number_ProductPage_URL";"https://www.icotek.com/en/products/hygienic-design-cable-entry-plates/kel-dpu-hd?tab=81374#variant-82794";"";
"Clamping_range_1_min";"3.2 mm";"";
"DESIGN";"KEL-DPU-HD 24|21";"";
"Width";"58 mm";"";
"For_min_wall_thickness";"1.5 mm";"";
"TraceParts.PartNumber";"90-23052025-045160";"";
"No_of_screw_holes";"4";"";
"t_max";"80 C°";"";
"Clamping_range_3_max";"10.5 mm";"";
"Clamping_range_5_amount";"";"";
"Flame_class";"UL94-HB";"";
"Thread";"M4";"";
"Material_base_frame";"Polypropylene";"";
"Clamping_range_5_max";"";"";
"Clamping_range_5_min";"";"";
"Cut_out_size";"112 × 36 mm";"";
"Material";"Elastomer";"";
"t_min";"-40 C°";"";
"TraceParts.PartVersion";"1.0.0";"";
"For_max_wall_thickness";"2 mm";"";
"TraceParts.PartLanguage";"en";"";
"Screw_hole_d";"4 mm";"";
"TRACEPARTS";"TRACEPARTS";"";
"Colour";"blue (similar RAL 5005)";"";
